(module russian-nixies-IN-12 (layer F.Cu) (tedit 60E543D2)
  (descr "MAY BE USED WITH SOCKET: SK-136")
  (tags "MAY BE USED WITH SOCKET: SK-136")
  (attr virtual)
  (fp_text reference >NAME (at 0 -13 180) (layer B.SilkS)
    (effects (font (size 1.27 1.27) (thickness 0.0889)))
  )
  (fp_text value Val** (at 9 0 90) (layer F.SilkS)
    (effects (font (size 1.524 1.524) (thickness 0.15)))
  )
  (fp_line (start 11 -11) (end 11 11) (layer F.SilkS) (width 0.15))
  (fp_line (start -11 11) (end -11 -11) (layer F.SilkS) (width 0.15))
  (fp_circle (center 0 0) (end 2 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 0) (end 3 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -3) (end 0 3) (layer F.SilkS) (width 0.15))
  (fp_arc (start 0 0) (end 11 11) (angle 90) (layer F.SilkS) (width 0.15))
  (fp_arc (start 0 0) (end -11 -11) (angle 90) (layer F.SilkS) (width 0.15))
  (pad 0 thru_hole circle (at 5.75 4.5) (size 3 3) (drill 1.6) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -4 8) (size 3 3) (drill 1.6) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -5.75 4.5) (size 3 3) (drill 1.6) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -5.75 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -5.75 -4.5) (size 3 3) (drill 1.6) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -4 -8) (size 3 3) (drill 1.6) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 -9) (size 3 3) (drill 1.6) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 4 -8) (size 3 3) (drill 1.6) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 5.75 -4.5) (size 3 3) (drill 1.6) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 5.75 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask))
  (pad A thru_hole circle (at 4 8) (size 3 3) (drill 1.6) (layers *.Cu *.Mask))
  (model ./IN-12B.wrl
    (offset (xyz 3.809999942779541 -7.619999885559082 7.619999885559082))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
