(export (version D)
  (design
    (source /home/lauri/nixiesp12/nixiesp.sch)
    (date "L 22 dets  2018 18:27:34 EET")
    (tool "Eeschema 4.0.7")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title NixiESP12)
        (company "Lauri Võsandi")
        (rev)
        (date 2017-07-13)
        (source nixiesp.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U5)
      (value 74HC595)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74xx) (part 74HC595))
      (sheetpath (names /) (tstamps /))
      (tstamp 59217C2D))
    (comp (ref N4)
      (value HH:XM:SS)
      (footprint nixiesp:russian-nixies-IN-12)
      (libsource (lib russian-nixies) (part IN-12A))
      (sheetpath (names /) (tstamps /))
      (tstamp 59219102))
    (comp (ref N3)
      (value HH:MX:SS)
      (footprint nixiesp:russian-nixies-IN-12)
      (libsource (lib russian-nixies) (part IN-12A))
      (sheetpath (names /) (tstamps /))
      (tstamp 592191F2))
    (comp (ref N5)
      (value HH:MM:SX)
      (footprint nixiesp:russian-nixies-IN-12)
      (libsource (lib russian-nixies) (part IN-12A))
      (sheetpath (names /) (tstamps /))
      (tstamp 5921FC78))
    (comp (ref N6)
      (value HH:MM:XS)
      (footprint nixiesp:russian-nixies-IN-12)
      (libsource (lib russian-nixies) (part IN-12A))
      (sheetpath (names /) (tstamps /))
      (tstamp 5921FE00))
    (comp (ref U8)
      (value 74HC595)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74xx) (part 74HC595))
      (sheetpath (names /) (tstamps /))
      (tstamp 5921FF85))
    (comp (ref J2)
      (value ESP8266)
      (footprint Socket_Strips:Socket_Strip_Straight_2x04_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_02X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 592253DB))
    (comp (ref N2)
      (value XH:MM:SS)
      (footprint nixiesp:russian-nixies-IN-12)
      (libsource (lib russian-nixies) (part IN-12A))
      (sheetpath (names /) (tstamps /))
      (tstamp 592192B4))
    (comp (ref Q2)
      (value BS107)
      (footprint TO_SOT_Packages_THT:TO-92_Inline_Wide)
      (libsource (lib nixiesp-rescue) (part BS107-RESCUE-nixiesp))
      (sheetpath (names /) (tstamps /))
      (tstamp 592AC4C6))
    (comp (ref Q1)
      (value BS107)
      (footprint TO_SOT_Packages_THT:TO-92_Inline_Wide)
      (libsource (lib nixiesp-rescue) (part BS107-RESCUE-nixiesp))
      (sheetpath (names /) (tstamps /))
      (tstamp 592ACDBD))
    (comp (ref R8)
      (value 15k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592AD40C))
    (comp (ref R7)
      (value 15k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592AD4D5))
    (comp (ref Q4)
      (value BS107)
      (footprint TO_SOT_Packages_THT:TO-92_Inline_Wide)
      (libsource (lib nixiesp-rescue) (part BS107-RESCUE-nixiesp))
      (sheetpath (names /) (tstamps /))
      (tstamp 592B0CA4))
    (comp (ref R9)
      (value 15k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592B1199))
    (comp (ref R10)
      (value 15k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592B12F4))
    (comp (ref N1)
      (value HX:MM:SS)
      (footprint nixiesp:russian-nixies-IN-12)
      (libsource (lib russian-nixies) (part IN-12A))
      (sheetpath (names /) (tstamps /))
      (tstamp 59219309))
    (comp (ref R11)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592AD7D9))
    (comp (ref R12)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592AE63C))
    (comp (ref R13)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592AE6EF))
    (comp (ref R14)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592AE7DF))
    (comp (ref R15)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592AE91A))
    (comp (ref R16)
      (value 10k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 592AE9E2))
    (comp (ref J1)
      (value "Power 9-15V")
      (footprint Connectors_Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol)
      (libsource (lib nixiesp-cache) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 592B31AF))
    (comp (ref U7)
      (value K155ID1)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74141) (part 74141-DIP))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BC62A))
    (comp (ref N7)
      (value IN-6)
      (footprint nixiesp:russian-nixies-IN-6)
      (libsource (lib russian-nixies) (part IN-6))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BEC1C))
    (comp (ref N10)
      (value IN-6)
      (footprint nixiesp:russian-nixies-IN-6)
      (libsource (lib russian-nixies) (part IN-6))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF0B0))
    (comp (ref N9)
      (value IN-6)
      (footprint nixiesp:russian-nixies-IN-6)
      (libsource (lib russian-nixies) (part IN-6))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF164))
    (comp (ref N8)
      (value IN-6)
      (footprint nixiesp:russian-nixies-IN-6)
      (libsource (lib russian-nixies) (part IN-6))
      (sheetpath (names /) (tstamps /))
      (tstamp 592BF578))
    (comp (ref U9)
      (value K155ID1)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74141) (part 74141-DIP))
      (sheetpath (names /) (tstamps /))
      (tstamp 592F06C2))
    (comp (ref J9)
      (value CONN_01X05)
      (footprint Socket_Strips:Socket_Strip_Straight_1x05_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X05))
      (sheetpath (names /) (tstamps /))
      (tstamp 593FFF9F))
    (comp (ref U12)
      (value LM1117-3.3)
      (footprint TO_SOT_Packages_SMD:SOT-223)
      (libsource (lib nixiesp-rescue) (part LM1117-3.3-RESCUE-nixiesp))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952D1A4))
    (comp (ref U10)
      (value LM1117-5.0)
      (footprint TO_SOT_Packages_SMD:SOT-223)
      (libsource (lib nixiesp-rescue) (part LM1117-5.0-RESCUE-nixiesp))
      (sheetpath (names /) (tstamps /))
      (tstamp 5952D692))
    (comp (ref U1)
      (value 74HC595)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74xx) (part 74HC595))
      (sheetpath (names /) (tstamps /))
      (tstamp 59219343))
    (comp (ref U11)
      (value 74HC595)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74xx) (part 74HC595))
      (sheetpath (names /) (tstamps /))
      (tstamp 59539D8E))
    (comp (ref U13)
      (value 74HC595)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74xx) (part 74HC595))
      (sheetpath (names /) (tstamps /))
      (tstamp 5955908F))
    (comp (ref J15)
      (value CONN_01X01)
      (footprint Connectors:1pin)
      (libsource (lib nixiesp-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59561B47))
    (comp (ref J16)
      (value CONN_01X01)
      (footprint Connectors:1pin)
      (libsource (lib nixiesp-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59561B4D))
    (comp (ref J17)
      (value CONN_01X01)
      (footprint Connectors:1pin)
      (libsource (lib nixiesp-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59561B53))
    (comp (ref J18)
      (value CONN_01X01)
      (footprint Connectors:1pin)
      (libsource (lib nixiesp-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59561B59))
    (comp (ref J19)
      (value CONN_01X01)
      (footprint Connectors:1pin)
      (libsource (lib nixiesp-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59561CC3))
    (comp (ref J20)
      (value CONN_01X01)
      (footprint Connectors:1pin)
      (libsource (lib nixiesp-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 59561CC9))
    (comp (ref J21)
      (value CONN_01X01)
      (footprint Connectors:1pin)
      (libsource (lib nixiesp-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 595728DA))
    (comp (ref J23)
      (value CONN_01X01)
      (footprint Connectors:1pin)
      (libsource (lib nixiesp-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 595728E6))
    (comp (ref J24)
      (value CONN_01X01)
      (footprint Connectors:1pin)
      (libsource (lib nixiesp-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 595728EC))
    (comp (ref J25)
      (value CONN_01X01)
      (footprint Connectors:1pin)
      (libsource (lib nixiesp-cache) (part CONN_01X01))
      (sheetpath (names /) (tstamps /))
      (tstamp 595728F2))
    (comp (ref J13)
      (value CONN_01X07)
      (footprint Pin_Headers:Pin_Header_Angled_1x07_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X07))
      (sheetpath (names /) (tstamps /))
      (tstamp 595BF0AC))
    (comp (ref U14)
      (value 74HC595)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74xx) (part 74HC595))
      (sheetpath (names /) (tstamps /))
      (tstamp 595C03E1))
    (comp (ref J12)
      (value CONN_01X06)
      (footprint Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 595C0883))
    (comp (ref U6)
      (value K155ID1)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74141) (part 74141-DIP))
      (sheetpath (names /) (tstamps /))
      (tstamp 595C2F35))
    (comp (ref U4)
      (value K155ID1)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74141) (part 74141-DIP))
      (sheetpath (names /) (tstamps /))
      (tstamp 595C3173))
    (comp (ref J10)
      (value CONN_01X06)
      (footprint Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 595C3185))
    (comp (ref U3)
      (value K155ID1)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74141) (part 74141-DIP))
      (sheetpath (names /) (tstamps /))
      (tstamp 595C364B))
    (comp (ref U2)
      (value K155ID1)
      (footprint Housings_DIP:DIP-16_W7.62mm)
      (libsource (lib 74141) (part 74141-DIP))
      (sheetpath (names /) (tstamps /))
      (tstamp 595C366A))
    (comp (ref J3)
      (value CONN_01X06)
      (footprint Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 595C367C))
    (comp (ref J5)
      (value CONN_01X06)
      (footprint Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 595BD9F2))
    (comp (ref J29)
      (value CONN_01X06)
      (footprint Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 595C1B86))
    (comp (ref J27)
      (value CONN_01X06)
      (footprint Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 595C37DE))
    (comp (ref J31)
      (value CONN_01X07)
      (footprint Socket_Strips:Socket_Strip_Straight_1x07_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X07))
      (sheetpath (names /) (tstamps /))
      (tstamp 595C3C2A))
    (comp (ref R1)
      (value 2.2k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 59692FCB))
    (comp (ref C1)
      (value C)
      (footprint Capacitors_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEBE841))
    (comp (ref C3)
      (value C)
      (footprint Capacitors_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEBEADC))
    (comp (ref C2)
      (value CP)
      (footprint Capacitors_THT:CP_Radial_D8.0mm_P3.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEBECC0))
    (comp (ref C4)
      (value CP)
      (footprint Capacitors_THT:CP_Radial_D8.0mm_P3.50mm)
      (libsource (lib device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEBEDBC))
    (comp (ref R2)
      (value 2.2k)
      (footprint Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BEC016E))
    (comp (ref J6)
      (value CONN_01X07)
      (footprint Pin_Headers:Pin_Header_Angled_1x07_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X07))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C1E4CB5))
    (comp (ref Q3)
      (value BS107)
      (footprint TO_SOT_Packages_THT:TO-92_Inline_Wide)
      (libsource (lib nixiesp-rescue) (part BS107-RESCUE-nixiesp))
      (sheetpath (names /) (tstamps /))
      (tstamp 592B0897))
    (comp (ref J11)
      (value CONN_01X07)
      (footprint Socket_Strips:Socket_Strip_Straight_1x07_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X07))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C1E5AB4))
    (comp (ref J14)
      (value CONN_01X07)
      (footprint Socket_Strips:Socket_Strip_Straight_1x07_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X07))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C1E73B8))
    (comp (ref J4)
      (value CONN_01X07)
      (footprint Pin_Headers:Pin_Header_Angled_1x07_Pitch2.54mm)
      (libsource (lib nixiesp-cache) (part CONN_01X07))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C1E785F)))
  (libparts
    (libpart (lib 74xx) (part 74HC595)
      (aliases
        (alias 74LS596)
        (alias 74LS595))
      (description "8 bits serial in // out Shift Register 3 State Out")
      (docs 74xx/74HC595.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 74HC595))
      (pins
        (pin (num 1) (name QB) (type 3state))
        (pin (num 2) (name QC) (type 3state))
        (pin (num 3) (name QD) (type 3state))
        (pin (num 4) (name QE) (type 3state))
        (pin (num 5) (name QF) (type 3state))
        (pin (num 6) (name QG) (type 3state))
        (pin (num 7) (name QH) (type 3state))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name ~QH) (type output))
        (pin (num 10) (name SRCLR) (type input))
        (pin (num 11) (name SRCLK) (type input))
        (pin (num 12) (name RCLK) (type input))
        (pin (num 13) (name G) (type input))
        (pin (num 14) (name SER) (type input))
        (pin (num 15) (name QA) (type 3state))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib nixiesp-rescue) (part BS107-RESCUE-nixiesp)
      (footprints
        (fp TO-92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BS107-RESCUE-nixiesp)
        (field (name Footprint) TO_SOT_Packages_THT:TO-92_Molded_Narrow))
      (pins
        (pin (num 1) (name D) (type passive))
        (pin (num 2) (name G) (type input))
        (pin (num 3) (name S) (type passive))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib nixiesp-cache) (part CONN_01X01)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X01))
      (pins
        (pin (num 1) (name P1) (type passive))))
    (libpart (lib nixiesp-cache) (part CONN_01X02)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib nixiesp-cache) (part CONN_01X05)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X05))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))))
    (libpart (lib nixiesp-cache) (part CONN_01X06)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))))
    (libpart (lib nixiesp-cache) (part CONN_01X07)
      (footprints
        (fp Pin_Header_Straight_1X*)
        (fp Pin_Header_Angled_1X*)
        (fp Socket_Strip_Straight_1X*)
        (fp Socket_Strip_Angled_1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_01X07))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))))
    (libpart (lib nixiesp-cache) (part CONN_02X04)
      (footprints
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*)
        (fp IDC_Header_Straight_*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_02X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib device) (part CP)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib 74141) (part Housings_DIP:DIP-16_W7.62mm)
      (aliases
        (alias 74141-DIP))
      (footprints
        (fp DIP-16))
      (fields
        (field (name Reference) U)
        (field (name Value) Housings_DIP:DIP-16_W7.62mm)
        (field (name Footprint) dip-sip:DIP-16))
      (pins
        (pin (num 1) (name 4) (type openCol))
        (pin (num 2) (name 2) (type openCol))
        (pin (num 3) (name A) (type input))
        (pin (num 4) (name D) (type input))
        (pin (num 5) (name VCC) (type power_in))
        (pin (num 6) (name B) (type input))
        (pin (num 7) (name C) (type input))
        (pin (num 8) (name 8) (type openCol))
        (pin (num 9) (name 9) (type openCol))
        (pin (num 10) (name 0) (type openCol))
        (pin (num 11) (name 7) (type openCol))
        (pin (num 12) (name GND) (type power_in))
        (pin (num 13) (name 6) (type openCol))
        (pin (num 14) (name 1) (type openCol))
        (pin (num 15) (name 3) (type openCol))
        (pin (num 16) (name 5) (type openCol))))
    (libpart (lib russian-nixies) (part IN-12A)
      (fields
        (field (name Reference) N)
        (field (name Value) IN-12A)
        (field (name Footprint) russian-nixies-IN-12))
      (pins
        (pin (num 0) (name 0) (type BiDi))
        (pin (num 1) (name 1) (type BiDi))
        (pin (num 2) (name 2) (type BiDi))
        (pin (num 3) (name 3) (type BiDi))
        (pin (num 4) (name 4) (type BiDi))
        (pin (num 5) (name 5) (type BiDi))
        (pin (num 6) (name 6) (type BiDi))
        (pin (num 7) (name 7) (type BiDi))
        (pin (num 8) (name 8) (type BiDi))
        (pin (num 9) (name 9) (type BiDi))
        (pin (num A) (name A) (type BiDi))))
    (libpart (lib russian-nixies) (part IN-6)
      (fields
        (field (name Reference) N)
        (field (name Value) IN-6)
        (field (name Footprint) russian-nixies-IN-6))
      (pins
        (pin (num A) (name A) (type BiDi))
        (pin (num K) (name K) (type BiDi))))
    (libpart (lib nixiesp-rescue) (part LM1117-3.3-RESCUE-nixiesp)
      (footprints
        (fp SOT-223*)
        (fp TO-263*)
        (fp TO-252*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-3.3-RESCUE-nixiesp))
      (pins
        (pin (num 1) (name GND/ADJ) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))
        (pin (num 4) (name VO) (type power_out))))
    (libpart (lib nixiesp-rescue) (part LM1117-5.0-RESCUE-nixiesp)
      (footprints
        (fp SOT-223*)
        (fp TO-263*)
        (fp TO-252*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-5.0-RESCUE-nixiesp))
      (pins
        (pin (num 1) (name GND/ADJ) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))
        (pin (num 4) (name VO) (type power_out))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical 74xx)
      (uri /usr/share/kicad/library/74xx.lib))
    (library (logical nixiesp-rescue)
      (uri nixiesp-rescue.lib))
    (library (logical 74141)
      (uri 74141.lib))
    (library (logical russian-nixies)
      (uri russian-nixies.lib))
    (library (logical nixiesp-cache)
      (uri /home/lauri/nixiesp12/nixiesp-cache.lib)))
  (nets
    (net (code 1) (name "Net-(J10-Pad1)")
      (node (ref J10) (pin 1))
      (node (ref Q2) (pin 2)))
    (net (code 2) (name "Net-(N8-PadA)")
      (node (ref N8) (pin A))
      (node (ref R7) (pin 2)))
    (net (code 3) (name "Net-(J11-Pad7)")
      (node (ref U1) (pin 1))
      (node (ref J11) (pin 7)))
    (net (code 4) (name "Net-(J5-Pad1)")
      (node (ref J5) (pin 1))
      (node (ref U1) (pin 2)))
    (net (code 5) (name "Net-(J12-Pad1)")
      (node (ref Q4) (pin 2))
      (node (ref J12) (pin 1)))
    (net (code 6) (name /data)
      (node (ref U8) (pin 14))
      (node (ref J2) (pin 3))
      (node (ref R2) (pin 2)))
    (net (code 7) (name "Net-(N10-PadK)")
      (node (ref N10) (pin K))
      (node (ref Q3) (pin 1)))
    (net (code 8) (name GND)
      (node (ref U12) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref U11) (pin 13))
      (node (ref J2) (pin 1))
      (node (ref U2) (pin 12))
      (node (ref J17) (pin 1))
      (node (ref U11) (pin 8))
      (node (ref J14) (pin 1))
      (node (ref U1) (pin 13))
      (node (ref J15) (pin 1))
      (node (ref U5) (pin 13))
      (node (ref J20) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref U3) (pin 12))
      (node (ref U10) (pin 1))
      (node (ref U5) (pin 8))
      (node (ref J23) (pin 1))
      (node (ref U4) (pin 12))
      (node (ref J31) (pin 1))
      (node (ref U8) (pin 13))
      (node (ref U14) (pin 8))
      (node (ref J13) (pin 1))
      (node (ref U14) (pin 13))
      (node (ref J25) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref J21) (pin 1))
      (node (ref U6) (pin 12))
      (node (ref J27) (pin 1))
      (node (ref U8) (pin 8))
      (node (ref J24) (pin 1))
      (node (ref U13) (pin 13))
      (node (ref J6) (pin 1))
      (node (ref Q3) (pin 3))
      (node (ref J11) (pin 1))
      (node (ref U13) (pin 8))
      (node (ref J16) (pin 1))
      (node (ref J18) (pin 1))
      (node (ref J19) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref U7) (pin 12))
      (node (ref J1) (pin 1))
      (node (ref J9) (pin 4))
      (node (ref Q2) (pin 3))
      (node (ref Q1) (pin 3))
      (node (ref Q4) (pin 3))
      (node (ref U9) (pin 12))
      (node (ref J9) (pin 2)))
    (net (code 9) (name "Net-(J6-Pad2)")
      (node (ref J6) (pin 2))
      (node (ref U6) (pin 7)))
    (net (code 10) (name "Net-(J6-Pad3)")
      (node (ref J6) (pin 3))
      (node (ref U6) (pin 6)))
    (net (code 11) (name "Net-(J6-Pad5)")
      (node (ref J6) (pin 5))
      (node (ref U6) (pin 4)))
    (net (code 12) (name "Net-(J6-Pad6)")
      (node (ref U6) (pin 3))
      (node (ref J6) (pin 6)))
    (net (code 13) (name "Net-(J6-Pad7)")
      (node (ref J6) (pin 7))
      (node (ref Q3) (pin 2)))
    (net (code 14) (name "Net-(J29-Pad1)")
      (node (ref U5) (pin 2))
      (node (ref J29) (pin 1)))
    (net (code 15) (name "Net-(J14-Pad6)")
      (node (ref J14) (pin 6))
      (node (ref U13) (pin 6)))
    (net (code 16) (name "Net-(J27-Pad2)")
      (node (ref U8) (pin 3))
      (node (ref J27) (pin 2)))
    (net (code 17) (name "Net-(J27-Pad3)")
      (node (ref J27) (pin 3))
      (node (ref U8) (pin 4)))
    (net (code 18) (name "Net-(J14-Pad5)")
      (node (ref J14) (pin 5))
      (node (ref U13) (pin 5)))
    (net (code 19) (name "Net-(J14-Pad3)")
      (node (ref J14) (pin 3))
      (node (ref U13) (pin 4)))
    (net (code 20) (name "Net-(J14-Pad2)")
      (node (ref J14) (pin 2))
      (node (ref U13) (pin 3)))
    (net (code 21) (name "Net-(J31-Pad3)")
      (node (ref U14) (pin 4))
      (node (ref J31) (pin 3)))
    (net (code 22) (name "Net-(J31-Pad7)")
      (node (ref J9) (pin 5))
      (node (ref J31) (pin 7)))
    (net (code 23) (name "Net-(J31-Pad6)")
      (node (ref J31) (pin 6))
      (node (ref U14) (pin 6)))
    (net (code 24) (name "Net-(J31-Pad5)")
      (node (ref U14) (pin 5))
      (node (ref J31) (pin 5)))
    (net (code 25) (name "Net-(J31-Pad2)")
      (node (ref J31) (pin 2))
      (node (ref U14) (pin 3)))
    (net (code 26) (name "Net-(J27-Pad6)")
      (node (ref U8) (pin 6))
      (node (ref J27) (pin 6)))
    (net (code 27) (name "Net-(J27-Pad5)")
      (node (ref U8) (pin 5))
      (node (ref J27) (pin 5)))
    (net (code 28) (name "Net-(N5-Pad6)")
      (node (ref U2) (pin 13))
      (node (ref N5) (pin 6)))
    (net (code 29) (name "Net-(N5-Pad1)")
      (node (ref N5) (pin 1))
      (node (ref U2) (pin 14)))
    (net (code 30) (name "Net-(N5-Pad3)")
      (node (ref N5) (pin 3))
      (node (ref U2) (pin 15)))
    (net (code 31) (name "Net-(N5-Pad4)")
      (node (ref N5) (pin 4))
      (node (ref U2) (pin 16)))
    (net (code 32) (name VCC)
      (node (ref U5) (pin 16))
      (node (ref U13) (pin 10))
      (node (ref U7) (pin 5))
      (node (ref U9) (pin 5))
      (node (ref U13) (pin 16))
      (node (ref U8) (pin 10))
      (node (ref U4) (pin 5))
      (node (ref U3) (pin 5))
      (node (ref J10) (pin 4))
      (node (ref J13) (pin 4))
      (node (ref U14) (pin 10))
      (node (ref U14) (pin 16))
      (node (ref J12) (pin 4))
      (node (ref U10) (pin 4))
      (node (ref U10) (pin 2))
      (node (ref U5) (pin 10))
      (node (ref U6) (pin 5))
      (node (ref U12) (pin 4))
      (node (ref U12) (pin 2))
      (node (ref U11) (pin 16))
      (node (ref U11) (pin 10))
      (node (ref J2) (pin 4))
      (node (ref J2) (pin 6))
      (node (ref J2) (pin 8))
      (node (ref U8) (pin 16))
      (node (ref U1) (pin 16))
      (node (ref U1) (pin 10))
      (node (ref C4) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref J29) (pin 4))
      (node (ref J31) (pin 4))
      (node (ref R1) (pin 2))
      (node (ref U2) (pin 5))
      (node (ref J4) (pin 4))
      (node (ref J14) (pin 4))
      (node (ref J27) (pin 4))
      (node (ref J5) (pin 4))
      (node (ref J3) (pin 4))
      (node (ref J11) (pin 4))
      (node (ref J6) (pin 4))
      (node (ref R2) (pin 1)))
    (net (code 33) (name "Net-(J3-Pad5)")
      (node (ref J3) (pin 5))
      (node (ref U2) (pin 4)))
    (net (code 34) (name "Net-(J5-Pad5)")
      (node (ref U1) (pin 5))
      (node (ref J5) (pin 5)))
    (net (code 35) (name "Net-(N5-Pad5)")
      (node (ref N5) (pin 5))
      (node (ref U2) (pin 1)))
    (net (code 36) (name "Net-(N6-Pad0)")
      (node (ref N6) (pin 0))
      (node (ref U3) (pin 10)))
    (net (code 37) (name "Net-(N6-Pad7)")
      (node (ref N6) (pin 7))
      (node (ref U3) (pin 11)))
    (net (code 38) (name "Net-(N6-Pad6)")
      (node (ref U3) (pin 13))
      (node (ref N6) (pin 6)))
    (net (code 39) (name "Net-(N6-Pad1)")
      (node (ref N6) (pin 1))
      (node (ref U3) (pin 14)))
    (net (code 40) (name "Net-(N6-Pad3)")
      (node (ref N6) (pin 3))
      (node (ref U3) (pin 15)))
    (net (code 41) (name "Net-(N6-Pad4)")
      (node (ref N6) (pin 4))
      (node (ref U3) (pin 16)))
    (net (code 42) (name "Net-(N5-Pad2)")
      (node (ref N5) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 43) (name "Net-(J3-Pad6)")
      (node (ref U2) (pin 3))
      (node (ref J3) (pin 6)))
    (net (code 44) (name "Net-(J3-Pad3)")
      (node (ref J3) (pin 3))
      (node (ref U2) (pin 6)))
    (net (code 45) (name "Net-(J3-Pad2)")
      (node (ref J3) (pin 2))
      (node (ref U2) (pin 7)))
    (net (code 46) (name "Net-(N5-Pad8)")
      (node (ref N5) (pin 8))
      (node (ref U2) (pin 8)))
    (net (code 47) (name "Net-(N5-Pad9)")
      (node (ref N5) (pin 9))
      (node (ref U2) (pin 9)))
    (net (code 48) (name "Net-(N5-Pad0)")
      (node (ref N5) (pin 0))
      (node (ref U2) (pin 10)))
    (net (code 49) (name "Net-(N5-Pad7)")
      (node (ref N5) (pin 7))
      (node (ref U2) (pin 11)))
    (net (code 50) (name "Net-(J29-Pad6)")
      (node (ref J29) (pin 6))
      (node (ref U5) (pin 6)))
    (net (code 51) (name "Net-(J1-Pad2)")
      (node (ref J9) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref U10) (pin 3))
      (node (ref U12) (pin 3)))
    (net (code 52) (name "Net-(N6-Pad5)")
      (node (ref N6) (pin 5))
      (node (ref U3) (pin 1)))
    (net (code 53) (name "Net-(N4-Pad5)")
      (node (ref U6) (pin 1))
      (node (ref N4) (pin 5)))
    (net (code 54) (name "Net-(N4-Pad6)")
      (node (ref N4) (pin 6))
      (node (ref U6) (pin 13)))
    (net (code 55) (name "Net-(N4-Pad7)")
      (node (ref N4) (pin 7))
      (node (ref U6) (pin 11)))
    (net (code 56) (name "Net-(N4-Pad0)")
      (node (ref U6) (pin 10))
      (node (ref N4) (pin 0)))
    (net (code 57) (name "Net-(N2-Pad1)")
      (node (ref U9) (pin 14))
      (node (ref N2) (pin 1)))
    (net (code 58) (name "Net-(N2-Pad2)")
      (node (ref U9) (pin 2))
      (node (ref N2) (pin 2)))
    (net (code 59) (name "Net-(N2-Pad3)")
      (node (ref U9) (pin 15))
      (node (ref N2) (pin 3)))
    (net (code 60) (name "Net-(N2-Pad0)")
      (node (ref U9) (pin 10))
      (node (ref N2) (pin 0)))
    (net (code 61) (name "Net-(N6-Pad2)")
      (node (ref N6) (pin 2))
      (node (ref U3) (pin 2)))
    (net (code 62) (name "Net-(J13-Pad7)")
      (node (ref R10) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref R13) (pin 1))
      (node (ref R8) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref J13) (pin 7))
      (node (ref R9) (pin 1))
      (node (ref R16) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref R12) (pin 1)))
    (net (code 63) (name "Net-(J14-Pad7)")
      (node (ref J14) (pin 7))
      (node (ref U5) (pin 1)))
    (net (code 64) (name "Net-(J4-Pad2)")
      (node (ref U3) (pin 7))
      (node (ref J4) (pin 2)))
    (net (code 65) (name "Net-(J4-Pad3)")
      (node (ref U3) (pin 6))
      (node (ref J4) (pin 3)))
    (net (code 66) (name "Net-(J4-Pad5)")
      (node (ref J4) (pin 5))
      (node (ref U3) (pin 4)))
    (net (code 67) (name "Net-(J4-Pad6)")
      (node (ref J4) (pin 6))
      (node (ref U3) (pin 3)))
    (net (code 68) (name "Net-(J4-Pad7)")
      (node (ref J4) (pin 7))
      (node (ref Q1) (pin 2)))
    (net (code 69) (name "Net-(U11-Pad14)")
      (node (ref U5) (pin 9))
      (node (ref U11) (pin 14)))
    (net (code 70) (name "Net-(N4-Pad8)")
      (node (ref N4) (pin 8))
      (node (ref U6) (pin 8)))
    (net (code 71) (name "Net-(N4-Pad9)")
      (node (ref U6) (pin 9))
      (node (ref N4) (pin 9)))
    (net (code 72) (name "Net-(N2-Pad9)")
      (node (ref U9) (pin 9))
      (node (ref N2) (pin 9)))
    (net (code 73) (name "Net-(N2-Pad8)")
      (node (ref U9) (pin 8))
      (node (ref N2) (pin 8)))
    (net (code 74) (name "Net-(N2-Pad7)")
      (node (ref N2) (pin 7))
      (node (ref U9) (pin 11)))
    (net (code 75) (name "Net-(N2-Pad6)")
      (node (ref N2) (pin 6))
      (node (ref U9) (pin 13)))
    (net (code 76) (name "Net-(N2-Pad5)")
      (node (ref U9) (pin 1))
      (node (ref N2) (pin 5)))
    (net (code 77) (name "Net-(N2-Pad4)")
      (node (ref U9) (pin 16))
      (node (ref N2) (pin 4)))
    (net (code 78) (name "Net-(N6-Pad9)")
      (node (ref N6) (pin 9))
      (node (ref U3) (pin 9)))
    (net (code 79) (name "Net-(N6-Pad8)")
      (node (ref N6) (pin 8))
      (node (ref U3) (pin 8)))
    (net (code 80) (name "Net-(N4-Pad4)")
      (node (ref N4) (pin 4))
      (node (ref U6) (pin 16)))
    (net (code 81) (name "Net-(U1-Pad14)")
      (node (ref U11) (pin 9))
      (node (ref U1) (pin 14)))
    (net (code 82) (name "Net-(U13-Pad14)")
      (node (ref U8) (pin 9))
      (node (ref U13) (pin 14)))
    (net (code 83) (name "Net-(U13-Pad9)")
      (node (ref U13) (pin 9))
      (node (ref U5) (pin 14)))
    (net (code 84) (name "Net-(J5-Pad3)")
      (node (ref J5) (pin 3))
      (node (ref U1) (pin 4)))
    (net (code 85) (name "Net-(J5-Pad2)")
      (node (ref J5) (pin 2))
      (node (ref U1) (pin 3)))
    (net (code 86) (name "Net-(J10-Pad5)")
      (node (ref J10) (pin 5))
      (node (ref U4) (pin 4)))
    (net (code 87) (name "Net-(J11-Pad5)")
      (node (ref U11) (pin 5))
      (node (ref J11) (pin 5)))
    (net (code 88) (name "Net-(J29-Pad5)")
      (node (ref J29) (pin 5))
      (node (ref U5) (pin 5)))
    (net (code 89) (name "Net-(J29-Pad3)")
      (node (ref J29) (pin 3))
      (node (ref U5) (pin 4)))
    (net (code 90) (name "Net-(J29-Pad2)")
      (node (ref J29) (pin 2))
      (node (ref U5) (pin 3)))
    (net (code 91) (name "Net-(J11-Pad6)")
      (node (ref J11) (pin 6))
      (node (ref U11) (pin 6)))
    (net (code 92) (name "Net-(J10-Pad6)")
      (node (ref U4) (pin 3))
      (node (ref J10) (pin 6)))
    (net (code 93) (name "Net-(J11-Pad3)")
      (node (ref J11) (pin 3))
      (node (ref U11) (pin 4)))
    (net (code 94) (name "Net-(J11-Pad2)")
      (node (ref U11) (pin 3))
      (node (ref J11) (pin 2)))
    (net (code 95) (name "Net-(J5-Pad6)")
      (node (ref U1) (pin 6))
      (node (ref J5) (pin 6)))
    (net (code 96) (name "Net-(U1-Pad9)")
      (node (ref U14) (pin 14))
      (node (ref U1) (pin 9)))
    (net (code 97) (name "Net-(N4-Pad1)")
      (node (ref U6) (pin 14))
      (node (ref N4) (pin 1)))
    (net (code 98) (name "Net-(N4-Pad2)")
      (node (ref N4) (pin 2))
      (node (ref U6) (pin 2)))
    (net (code 99) (name "Net-(N4-Pad3)")
      (node (ref N4) (pin 3))
      (node (ref U6) (pin 15)))
    (net (code 100) (name "Net-(J13-Pad5)")
      (node (ref U9) (pin 4))
      (node (ref J13) (pin 5)))
    (net (code 101) (name "Net-(J10-Pad3)")
      (node (ref J10) (pin 3))
      (node (ref U4) (pin 6)))
    (net (code 102) (name "Net-(J10-Pad2)")
      (node (ref J10) (pin 2))
      (node (ref U4) (pin 7)))
    (net (code 103) (name "Net-(J13-Pad6)")
      (node (ref U9) (pin 3))
      (node (ref J13) (pin 6)))
    (net (code 104) (name "Net-(J13-Pad3)")
      (node (ref U9) (pin 6))
      (node (ref J13) (pin 3)))
    (net (code 105) (name "Net-(J13-Pad2)")
      (node (ref U9) (pin 7))
      (node (ref J13) (pin 2)))
    (net (code 106) (name "Net-(J12-Pad5)")
      (node (ref U7) (pin 4))
      (node (ref J12) (pin 5)))
    (net (code 107) (name "Net-(J12-Pad6)")
      (node (ref J12) (pin 6))
      (node (ref U7) (pin 3)))
    (net (code 108) (name "Net-(J12-Pad3)")
      (node (ref J12) (pin 3))
      (node (ref U7) (pin 6)))
    (net (code 109) (name "Net-(J12-Pad2)")
      (node (ref J12) (pin 2))
      (node (ref U7) (pin 7)))
    (net (code 110) (name "Net-(N7-PadA)")
      (node (ref N7) (pin A))
      (node (ref R10) (pin 2)))
    (net (code 111) (name "Net-(N1-Pad0)")
      (node (ref U7) (pin 10))
      (node (ref N1) (pin 0)))
    (net (code 112) (name "Net-(N1-Pad1)")
      (node (ref N1) (pin 1))
      (node (ref U7) (pin 14)))
    (net (code 113) (name "Net-(N1-Pad2)")
      (node (ref U7) (pin 2))
      (node (ref N1) (pin 2)))
    (net (code 114) (name "Net-(N1-Pad3)")
      (node (ref U7) (pin 15))
      (node (ref N1) (pin 3)))
    (net (code 115) (name "Net-(N1-Pad4)")
      (node (ref U7) (pin 16))
      (node (ref N1) (pin 4)))
    (net (code 116) (name "Net-(N1-Pad5)")
      (node (ref U7) (pin 1))
      (node (ref N1) (pin 5)))
    (net (code 117) (name "Net-(N1-Pad6)")
      (node (ref U7) (pin 13))
      (node (ref N1) (pin 6)))
    (net (code 118) (name "Net-(N1-Pad7)")
      (node (ref N1) (pin 7))
      (node (ref U7) (pin 11)))
    (net (code 119) (name "Net-(N1-Pad8)")
      (node (ref N1) (pin 8))
      (node (ref U7) (pin 8)))
    (net (code 120) (name "Net-(N1-Pad9)")
      (node (ref U7) (pin 9))
      (node (ref N1) (pin 9)))
    (net (code 121) (name "Net-(N1-PadA)")
      (node (ref N1) (pin A))
      (node (ref R15) (pin 2)))
    (net (code 122) (name "Net-(N10-PadA)")
      (node (ref R9) (pin 2))
      (node (ref N10) (pin A)))
    (net (code 123) (name "Net-(N5-PadA)")
      (node (ref N5) (pin A))
      (node (ref R11) (pin 2)))
    (net (code 124) (name "Net-(N6-PadA)")
      (node (ref R12) (pin 2))
      (node (ref N6) (pin A)))
    (net (code 125) (name "Net-(N3-PadA)")
      (node (ref R13) (pin 2))
      (node (ref N3) (pin A)))
    (net (code 126) (name "Net-(N4-PadA)")
      (node (ref R14) (pin 2))
      (node (ref N4) (pin A)))
    (net (code 127) (name "Net-(N2-PadA)")
      (node (ref R16) (pin 2))
      (node (ref N2) (pin A)))
    (net (code 128) (name "Net-(N8-PadK)")
      (node (ref Q1) (pin 1))
      (node (ref N8) (pin K)))
    (net (code 129) (name "Net-(N9-PadK)")
      (node (ref Q2) (pin 1))
      (node (ref N9) (pin K)))
    (net (code 130) (name "Net-(N9-PadA)")
      (node (ref N9) (pin A))
      (node (ref R8) (pin 2)))
    (net (code 131) (name "Net-(N7-PadK)")
      (node (ref N7) (pin K))
      (node (ref Q4) (pin 1)))
    (net (code 132) (name "Net-(J9-Pad3)")
      (node (ref J9) (pin 3)))
    (net (code 134) (name "Net-(N3-Pad0)")
      (node (ref U4) (pin 10))
      (node (ref N3) (pin 0)))
    (net (code 135) (name "Net-(N3-Pad1)")
      (node (ref N3) (pin 1))
      (node (ref U4) (pin 14)))
    (net (code 136) (name "Net-(N3-Pad2)")
      (node (ref N3) (pin 2))
      (node (ref U4) (pin 2)))
    (net (code 137) (name "Net-(N3-Pad3)")
      (node (ref N3) (pin 3))
      (node (ref U4) (pin 15)))
    (net (code 138) (name "Net-(N3-Pad4)")
      (node (ref N3) (pin 4))
      (node (ref U4) (pin 16)))
    (net (code 139) (name "Net-(N3-Pad5)")
      (node (ref N3) (pin 5))
      (node (ref U4) (pin 1)))
    (net (code 140) (name "Net-(N3-Pad6)")
      (node (ref U4) (pin 13))
      (node (ref N3) (pin 6)))
    (net (code 141) (name "Net-(N3-Pad7)")
      (node (ref U4) (pin 11))
      (node (ref N3) (pin 7)))
    (net (code 142) (name "Net-(N3-Pad8)")
      (node (ref U4) (pin 8))
      (node (ref N3) (pin 8)))
    (net (code 143) (name "Net-(N3-Pad9)")
      (node (ref U4) (pin 9))
      (node (ref N3) (pin 9)))
    (net (code 144) (name "Net-(U5-Pad7)")
      (node (ref U5) (pin 7)))
    (net (code 145) (name "Net-(U5-Pad15)")
      (node (ref U5) (pin 15)))
    (net (code 146) (name "Net-(J2-Pad2)")
      (node (ref J2) (pin 2)))
    (net (code 147) (name "Net-(U8-Pad1)")
      (node (ref U8) (pin 1)))
    (net (code 148) (name "Net-(U8-Pad2)")
      (node (ref U8) (pin 2)))
    (net (code 149) (name "Net-(U8-Pad7)")
      (node (ref U8) (pin 7)))
    (net (code 150) (name "Net-(U8-Pad15)")
      (node (ref U8) (pin 15)))
    (net (code 151) (name "Net-(U14-Pad7)")
      (node (ref U14) (pin 7)))
    (net (code 152) (name "Net-(U14-Pad9)")
      (node (ref U14) (pin 9)))
    (net (code 153) (name "Net-(U14-Pad15)")
      (node (ref U14) (pin 15)))
    (net (code 155) (name "Net-(U14-Pad1)")
      (node (ref U14) (pin 1)))
    (net (code 156) (name "Net-(U14-Pad2)")
      (node (ref U14) (pin 2)))
    (net (code 158) (name "Net-(U1-Pad15)")
      (node (ref U1) (pin 15)))
    (net (code 159) (name "Net-(U11-Pad1)")
      (node (ref U11) (pin 1)))
    (net (code 160) (name "Net-(U11-Pad2)")
      (node (ref U11) (pin 2)))
    (net (code 161) (name "Net-(U11-Pad7)")
      (node (ref U11) (pin 7)))
    (net (code 162) (name "Net-(U11-Pad15)")
      (node (ref U11) (pin 15)))
    (net (code 163) (name /latch)
      (node (ref R1) (pin 1))
      (node (ref J2) (pin 5))
      (node (ref U5) (pin 12))
      (node (ref U13) (pin 12))
      (node (ref U14) (pin 12))
      (node (ref U11) (pin 12))
      (node (ref U1) (pin 12))
      (node (ref U8) (pin 12)))
    (net (code 164) (name /clock)
      (node (ref U1) (pin 11))
      (node (ref U13) (pin 11))
      (node (ref U5) (pin 11))
      (node (ref U11) (pin 11))
      (node (ref U14) (pin 11))
      (node (ref U8) (pin 11))
      (node (ref J2) (pin 7)))
    (net (code 165) (name "Net-(U1-Pad7)")
      (node (ref U1) (pin 7)))
    (net (code 167) (name "Net-(U13-Pad1)")
      (node (ref U13) (pin 1)))
    (net (code 168) (name "Net-(U13-Pad2)")
      (node (ref U13) (pin 2)))
    (net (code 169) (name "Net-(U13-Pad7)")
      (node (ref U13) (pin 7)))
    (net (code 170) (name "Net-(U13-Pad15)")
      (node (ref U13) (pin 15)))))